*Table 1*

|  |  |  |  |
| --- | --- | --- | --- |
| **Synchronous areas** | **Range for the maximum capacity threshold from which a power-generating module is of type B** | **Range for the maximum capacity threshold from which a power-generating module is of type C** | **Range for the maximum capacity threshold from which a power-generating module is of type D** |
| Continental Europe | 0.1 MW - 1 MW | 5 MW - 50 MW | 25 MW - 75 MW |
| Great Britain | 0.1 MW - 1 MW | 5 MW – 50 MW | 25 MW - 75 MW |
| Nordic | 0.1 MW - 1,5 MW | ? - 10 MW | ? - 30 MW |
| Ireland and Northern Ireland | 0.1 MW - 0,1 MW | ? - 5 MW | ? - 10 MW |
| Baltic | 0.1 MW - 0,5 MW | ? - 10 MW | ? - 15 MW |

**Ranges for thresholds for type B, C and D power-generating modules**