*Table 8*

**Parameters for the inner envelope in Figure 7**

|  |  |  |
| --- | --- | --- |
| **Synchronous area** | **Maximum range of Q/Pmax** | **Maximum range of steady-state voltage level in PU** |
| Continental Europe | 0.7 | 0.175 |
| Nordic | 0,95 | 0,150 |
| Great Britain | 0,95 | 0,225 |
| Ireland and Northern Ireland | 1,08 | 0,218 |
| Baltic | 1,0 | 0,220 |

As a consequence of the proposed diagram Fig.7